	WPC FUSE LIST
	CAUTION!
	For continued protection against risk of fire, replace only with the same type of fuse having the same ratings.
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	F501
	-25V
	3A, 250V, SB
	
	
	

	Power Driver Board
	F502
	+25V
	3A, 250V, SB
	
	
	

	F101
	+50V DC General (Lt. Flipper)
	3A, 250V, SB
	F109
	G.I. #2 White-Orange
	5A, 250V, SB
	Dot Matrix Controller Board
	
	
	

	F102
	+50V DC General (Rt. Flipper)
	3A, 250V, SB
	F110
	G.I. #1 White-Brown
	5A, 250V, SB
	F601
	3/8A, 250V, FB
	+62V
	
	
	

	F103
	Solenoids #25 to #28
	3A, 250V, SB
	F111
	Flasher Secondary
	5A, 250V, SB
	F602
	3/8A, 250V, FB
	-113V & -125V
	
	
	

	F104
	Solenoids #9 to #16
	3A, 250V, SB
	F112
	Solenoid Secondary 
	7A, 250V, SB
	Fliptronic II Controller Board
	
	
	

	F105
	Solenoids #1 to #8
	3A, 250V, SB
	F113
	+5V Logic
	5A, 250V, SB
	F901
	3A, 250V, SB
	Upper Right Flipper
	
	
	

	F106
	G.I. #5 White-Violet
	5A, 250V, SB
	F114
	+18V Lamp Matrix
	8A, 32V, N.B.
	F902
	3A, 250V, SB
	Upper Left Flipper
	
	
	

	F107
	G.I. #4 White-Green
	5A, 250V, SB
	F115
	+12V Lamp Matrix
	3/4A, 250V, FB
	F903
	3A, 250V, SB
	Lower Right Flipper
	
	
	

	F108
	G.I. #3 White-Yellow
	5A, 250V, SB
	F116
	+12V Secondary
	3A, 250V, SB
	F904
	3A, 250V, SB
	Lower Left Flipper
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