FUSE LIST

CAUTION:
FOR CONTINUED PROTECTION AGAINST RISK OF FIRE, REPLACE ONLY WITH THE SAME TYPE OF FUSE HAVING THE SAME ELECTRICAL RATINGS.

ATTENTION:  UTILISER UN FUSIBLE DE RECHARGE DE MEME TYPE.
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AUDIO/VIDEO BOARD
	POWER DRIVER BOARD
	16-10137.5

	F501
	-25V
	T2.5A, 250V
	F101
	Regulated 12V
	T0.63A, 250V
	F110
	G.I. #5 White-Violet
	T4.0A, 250V

	F502
	+25V
	T2.5A, 250V
	F102
	Solenoids #25 to #28
	T4.0A, 250V
	F111
	G.I. #4 White-Green
	T4.0A, 250V

	F601
	+62V
	T0.315A, 250V
	F103
	Solenoids #1 to #8
	T4.0A, 250V
	F112
	G.I. #3 White-Yellow
	T4.0A, 250V

	F602
	-113V & -125V
	T0.315A, 250V
	F104
	Solenoids #9 to #16
	T4.0A, 250V
	F113
	G.I. #2 White-Orange
	T4.0A, 250V

	
	
	
	F105
	+5V Logic
	T4.0A, 250V
	F114
	G.I. #1 White-Brown
	T4.0A, 250V

	
	
	
	F106
	+18V Lamp Matrix
	T5.0A, 250V
	F115
	+50V Flippers
	T4.0A, 250V

	LINE FILTER
	
	F107
	Flasher Secondary
	T4.0A, 250V
	F116
	+50V Flippers
	T4.0A, 250V

	Foreign
	T4.0A, 250V
	F108
	Solenoid Secondary
	T6.3A, 250V
	F117
	+50V Flippers
	T4.0A, 250V

	Domestic
	T5.0A, 250V
	F109
	Unregulated 12V
	T4.0A, 250V
	F118
	+50V Flippers
	T4.0A, 250V
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