ARABIAN NIGHTS (50047)
                                      
FUSE LIST

	AUDIO/VIDEO BOARD
	POWER DRIVER BOARD

	F501
	-25V
	T2.5A, 250V
	F101
	Regulated 12V
	T0.63A, 250V
	F110
	G.I. #5 White-Violet
	T4.0A, 250V

	F502
	+25V
	T2.5A, 250V
	F102
	Solenoids #9 to #16
	T4.0A, 250V
	F111
	G.I. #4 White-Green
	T4.0A, 250V

	F601
	+62V
	T0.25A, 250V
	F103
	Solenoids #1 to #8
	T4.0A, 250V
	F112
	G.I. #3 White-Yellow
	T4.0A, 250V

	F602
	-113V & -125V
	T0.25A, 250V
	F104
	Solenoids #25 to #28
	T4.0A, 250V
	F113
	G.I. #2 White-Orange
	T4.0A, 250V

	
	
	
	F105
	+5V Logic
	T4.0A, 250V
	F114
	G.I. #1 White-Brown
	T4.0A, 250V

	
	
	
	F106
	+18V Lamp Matrix
	T5.0A, 250V
	F115
	+50V Flippers
	T4.0A, 250V

	LINE FILTER
	
	F107
	Flasher Secondary
	T4.0A, 250V
	F116
	+50V Flippers
	T4.0A, 250V

	Foreign
	T4.0A, 250V
	F108
	Solenoid Secondary
	T6.3A, 250V
	F117
	+50V Flippers
	T4.0A, 250V

	Domestic
	T5.0A, 250V
	F109
	Unregulated 12V
	T4.0A, 250V
	F118
	+50V Flippers
	T4.0A, 250V
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CAUTION: FOR CONTINUED PROTECTION

AGAINST RISK OF FIRE, REPLACE ONLY WITH

THE SAME TYPE OF FUSE HAVING THE SAME

ELECTRICAL RATINGS.

ATTENTION: UTILISER UN FUSIBLE DE

RECHARGE DE MEME TYPE.


SOLENOID/FLASHER TABLE

	Sol
No.
	Function
	Solenoid
Type
	Voltage Connections
	Drive
Xistor
	Drive Connections     
	Drive
Wire
Color
	Solenoid Part Number
Flashlamp Type

	
	
	
	Playfield
	Backbox
	Cabinet
	
	Playfield
	Backbox
	Cabinet
	
	Playfield
	Backbox

	01
	LEFT CAGE  
	High Power
	J133-2
	
	
	Q72
	J116-1
	
	
	VIO-BRN
	A-20099
	

	02
	RIGHT CAGE 
	High Power
	J133-2
	
	
	Q68
	J116-2
	
	
	VIO-RED
	A-20099
	

	03
	VANISH DROP
	High Power
	J133-2
	
	
	Q71
	J116-4
	
	
	VIO-ORG
	FL-11753
	

	04
	LOCK EJECT
	High Power
	J133-2
	
	
	Q67
	J116-5
	
	
	VIO-YEL
	AE-27-1200
	

	05
	BAZAAR EJECT
	High Power
	J133-2
	
	
	Q70
	J116-6
	
	
	VIO-GRN
	AE-25-1000
	

	06
	LOCK MAGNET
	High Power
	J133-2
	
	
	Q66
	J116-7
	
	
	VIO-BLU
	20-10197
	

	07
	KNOCKER 
	High Power
	
	J133-2
	
	Q69
	
	J116-8
	
	VIO-BLK
	
	AE-23-800

	08
	RAMP MAGNET COIL
	High Power
	J133-1
	
	
	Q65
	J116-9
	
	
	VIO-GRY
	20-10197
	

	09
	TROUGH EJECT
	Low Power
	J133-3
	
	
	Q44
	J113-1
	
	
	BRN-BLK
	AE-26-1500
	

	10
	LEFT SLINGSHOT
	Low Power
	J133-3
	
	
	Q48
	J113-3
	
	
	BRN-RED
	AE-27-1200
	

	11
	RIGHT SLINGSHOT
	Low Power
	J133-3
	
	
	Q43
	J113-4
	
	
	BRN-ORG
	AE-27-1200
	

	12
	LEFT JET BUMPER
	Low Power
	J133-3
	
	
	Q47
	J113-5
	
	
	BRN-YEL
	AE-26-1200
	

	13
	RIGHT JET BUMPER
	Low Power
	J133-3
	
	
	Q42
	J113-6
	
	
	BRN-GRN
	AE-26-1200
	

	14
	MIDDLE JET BUMPER
	Low Power
	J133-3
	
	
	Q46
	J113-7
	
	
	BRN-BLU
	AE-26-1200
	

	15
	LEFT KICKER
	Low Power
	J133-3
	
	
	Q41
	J113-8
	
	
	BRN-VIO
	AE-27-1200
	

	16
	LEFT EJECT FLASHER
	Low Power
	J133-6
	J134-5
	
	Q45
	J113-9
	J114-5
	
	BRN-GRY
	#89 (2)
	#906

	17
	INLANE FLASHERS
	Flasher
	J133-6
	
	
	Q28
	J111-1
	
	
	BLK-BRN
	#89 (2)
	

	18
	FINAL BATTLE FLASHER
	Flasher
	J133-6
	
	
	Q32
	J111-2
	
	
	BLK-RED
	#906
	

	19
	LEFT LOOP FLASHER
	Flasher
	J133-6
	
	
	Q27
	J111-3
	
	
	BLK-ORG
	#906
	

	20
	BAZAAR FLASHER
	Flasher
	J133-6
	
	
	Q31
	J111-4
	
	
	BLK-YEL
	#89
	

	21
	RAMP DIVERTOR
	Low Power
	J133-2
	
	
	Q26
	J111-5
	
	
	BLU-GRN
	AE-30-2000
	

	22
	RUB LAMP FLASHER
	Flasher
	J133-6
	
	
	Q30
	J111-6
	
	
	BLU-BLK
	#906
	

	23
	MAGIC LAMP FLASHERS
	Flasher
	J133-6
	
	
	Q25
	J111-7
	
	
	BLU-VIO
	#906
	

	24
	RIGHT LOOP FLASHER
	Flasher
	J133-6
	
	
	Q29
	J111-8
	
	
	BLU-GRY
	#906
	

	25
	START TALE FLASHERS
	Gen. Purpose
	J133-6
	J134-5
	
	Q16
	J109-1
	J108-1
	
	BLU-BRN
	#906
	#906

	26
	JET FLASHERS
	Gen. Purpose
	J133-6
	J134-5
	
	Q15
	J109-2
	J108-2
	
	BLU-RED
	#906
	#906

	27
	TOP LOOP FLASHER
	Gen. Purpose
	J133-6
	J134-5
	
	Q14
	J109-3
	J108-3
	
	BLU-ORG
	#906
	#906

	28
	RAMP FLASHER
	Gen. Purpose
	J133-6
	
	
	Q13
	J109-4
	
	
	BLU-YEL
	#906
	

	  General Illumination
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	01
	ILLUMINATION STRING 1
	G.I.
	
	J106-1
	
	Q5
	
	J105-7
	
	WHT-BRN
	#44
	

	02
	ILLUMINATION STRING 2
	G.I.
	
	J106-2
	
	Q4
	
	J105-8
	
	WHT-ORG
	#44
	

	03
	ILLUMINATION STRING 3
	G.I.
	
	J106-3
	
	Q3
	
	J105-9
	
	WHT-YEL
	#44
	

	04
	*ILLUMINATION STRING 4
	G.I.
	J105-5
	
	
	Q2
	J106-10
	
	
	WHT-GRN
	
	#555

	05
	*ILLUMINATION STRING 5
	G.I.
	J105-6
	
	J104-3
	Q1
	J106-11
	
	J104-1
	WHT-VIO
	
	#555

	  Flipper Circuits
	
	Voltage
Connection

Playfield
	Drive Transistors
	Drive

Connections
	Drive Wire

Colors
	Coil
Part No.
	Coil
Colors

	
	
	
	Power
	Hold
	Playfield
	Power                Hold
	
	

	29
	LOWER RIGHT FLIPPER
	Power
	J119-1 (RED-GRN)
	Q90
	
	J120-13
	YEL-GRN
	FL-11629
	BLUE

	30
	
	Hold
	J119-1 (RED-GRN)
	
	Q92
	J120-11
	ORG-GRN
	
	

	31
	LOWER LEFT FLIPPER
	Power
	J119-4 (RED-BLU)
	Q67
	
	J120-9
	YEL-BLU
	FL-11629
	BLUE

	32
	
	Hold
	J119-4 (RED-BLU)
	
	Q69
	J120-7
	ORG-BLU
	
	

	33
	LEFT DIVERTOR POWER

LEFT DIVERTOR HOLD
	Power
	J119-6 (RED-VIO)
	Q84
	
	J120-6
	YEL-VIO
	  FL-11753
	YELLOW

	34
	
	Hold
	J119-6 (RED-VIO
	
	Q86
	J120-4
	ORG-VIO
	
	

	35
	VANISH MAGNET

LOOP POST DIVERTOR
	Power
	J119-8 (RED-GRY)
	Q81
	
	J120-3
	YEL-GRY
	  20-10197
	

	36
	
	Hold
	J119-8 (RED-GRY)
	
	Q83
	J120-1
	ORG-GRY
	AE-27-1200
	


J1XX = POWER DRIVER BOARD

*These general illumination strings do not brighten and dim, they are always on


      LAMP MATRIX
Yellow (B+) 
Red
16-10213
	     Column

 Row
	1

Yellow-
Brown
J121-1

Q96
	2

Yellow-
Red
J121-2

Q100
	3

Yellow-
Orange
J121-3

Q95
	4

Yellow-
Black
J121-4

Q99
	5

Yellow-
Green
J121-5

Q94
	6

Yellow-
Blue
J121-6

Q98
	7

Yellow-
Violet
J121-7

Q93
	8

Yellow-
Grey
J121-8

Q97

	1

Red-
Brown
J125-1 Q104
	JEWEL 

1

(LEFT)

   11
	JACKPOT

21
	MAGIC
CARPET

  31
	SMOKE

6

41
	SMOKE

14

(TOP)

51
	MAKE A WISH

61
	ACTION

2

71
	EXTRA

BALL

81

	2

Red-
Black
J125-2 Q108
	JEWEL 

2


12
	(G)ENIE

22
	ACTION

3

32
	SMOKE

7

42
	LAMP-15

52
	(B)AZAAR

62
	LEFT

LOCK

72
	ACTION

5

82

	3

Red-
Orange
J125-4 Q103


	JEWEL
3

13
	G(E)NIE

23
	RAMP ARROW

RIGHT

33
	SMOKE
8


43
	LAMP-30

53
	B(A)ZAAR


63
	HAREM
ADVANCE

73
	RIGHT

LOCK

83

	4

Red-
Yellow
J125-5 Q107


	JEWEL
​4

14
	GE(N)IE



24
	RAMP ARROW
LEFT

34
	SMOKE
9

44
	LAMP-60

54
	BA(Z)AAR

64
	LEFT TIGER

LOOP

74
	RIGHT

TIGER

LOOP

84

	5

Red-
Green
J125-6 Q102


	JEWEL
5

15
	GEN(I)E
1

25
	SMOKE

1

(BOTTOM)

35
	SMOKE 

10

45
	SMOKE
​4

55
	BAZ(A)AR

65
	ACTION

1

75
	CAPTIVE

BALL

RIGHT

85

	6

Red-
​Blue
J125-7 Q106


	JEWEL
6

16
	GENI(E)


26
	SMOKE
2

36
	SMOKE

11

46
	SMOKE

5

56
	BAZA(A)R

66
	WISH

1

76
	ACTION
4

86

	7

Red​-
Violet
J125-8 Q101


	JEWEL

7

(RIGHT)

17
	MULTIBALL

27
	SMOKE
3

37
	SMOKE
12

47
	SHOOT
STAR
RIGHT

57
	BAZAA(R)

67
	WISH
2

77
	CAPTIVE

BALL

LEFT

87

	8

Red​-
Grey
J125-9 Q105


	SHOOT AGAIN

18
	OUTLANE

SPECIAL 

28
	AMULET 

38
	SMOKE

13

48
	SHOOT
STAR
LEFT

58
	CENTER

LOCK

68
	WISH

3

78
	START BUTTON

88


        J1XX = Power Driver Board

SWITCH MATRIX
White
Green
	DEDICATED
GROUNDED
SWITCHES
	    Column

Row
	1

Green-
Brown
J206-1

U20-18
	2

Green-
Red
J206-2

U20-17
	3

Green-
Orange
j206-3

U20-16
	4

Green-
Yellow
j206-4

U20-15
	5

Green-
Black
j206-5

U20-14
	6

Green-
Blue
J206-6

U20-13
	7

Green-
Violet
J206-7

U20-12
	8

Green-
Grey
J206-9

U20-11
	FLIPPER
GROUNDED

SWITCHES

	Orange-Brown
J205-1
LEFT COIN
CHUTE
U17-5

D1
	1

White-
Brown
J208-1

U18-11
	HAREM
PASSAGE

  11
	SLAM
TILT

21
	TROUGH
EJECT

  31
	RAMP
MADE

LEFT

41
	LEFT
SLING

51
	LEFT
STANDUPS


61
	NOT
USED

71
	NOT
USED 

81
	Black-Green
J208-13
Lower Right
Flipper E.O.S.

F1

	Orange-Red
J205-2
CENTER COIN
CHUTE
U17-7

D2
	2

White-
Red
J208-2

U18-9
	VANISH
TUNNEL


12
	COIN
DOOR
CLOSED

22
	TROUGH
BALL
1

32
	GENIE
TARGET


42
	RIGHT
SLING

52
	RIGHT
STANDUPS

62
	NOT
USED

72
	NOT
USED

82
	Blue-Violet
J212-12
Lower Right
Flipper Opto

F2

	Orange-Black
J205-3
RIGHT COIN
CHUTE
U17-11
D3
	3

White-
Orange
J208-3

U18-5
	START
BUTTON

13
	GENIE
STANDUP

TARGET

23
	TROUGH
BALL
2

33
	LEFT
LOOP

43
	LEFT
JET


53
	TOP
SKILL


63
	NOT
USED

73
	NOT
USED

83
	Black-Blue

J208-12

Lower Left
Flipper E.O.S.

F3

	Orange-Yellow
J205-4
4TH COIN
CHUTE
U17-9

D4
	4

White-
Yellow
J208-4

U18-7
	PLUMB
BOB
TILT

14
	ALWAYS
CLOSED

24
	TROUGH
BALL
3

34
	INNER
LOOP
LEFT

44
	RIGHT
JET


54
	MIDDLE
SKILL


64
	NOT
USED


74
	NOT
USED

84
	Blue-Gray

J212-11

Lower Left
Flipper Opto

F4

	Orange-Green
J205-6         U16-9
	5

White-
Green
J208-5

U19-11
	RAMP
ENTER


15
	BAZAAR
EJECT

25
	TROUGH
BALL
4

35
	INNER
LOOP
RIGHT

45
	MIDDLE
JET


55
	BOTTOM
SKILL

65
	NOT
USED


75
	NOT
USED

85
	Black-Violet

J208-11

Upper Right

Flipper E.O.S.

F5

	Normal  
Function
Srv Crdts
	Test Function

Escape
	
	
	
	
	
	
	
	
	
	

	D5
	
	
	
	
	
	
	
	
	
	

	Orange-Blue
J205-7          U16-11
	6

White-
​Blue
J208-7

U19-9
	LEFT
OUTLANE


16
	LEFT
INLANE

26
	LEFT
CAGE

OPTO

36
	MINI
STANDUPS


46
	LAMP SPIN
CCW


56
	LOCK 1
(BOTTOM)


66
	NOT
USED


76
	NOT
USED

86
	Black-Yellow
J212-10
Upper Right
Flipper Opto

F6

	Normal          

Function Volume Dn
	Test
Function

Down
	
	
	
	
	
	
	
	
	
	

	D6
	
	
	
	
	
	
	
	
	
	

	Orange-Violet
J205-8          U16-7
	7

White​-
Violet
J208-8

U19-5
	RIGHT
INLANE


17
	RIGHT
OUTLANE

27
	RIGHT

CAGE

OPTO

37
	RAMP
MADE

RIGHT


47
	LAMP SPIN
CW


57
	LOCK 2
(MIDDLE)


67
	NOT
USED


 77
	NOT
USED

87
	Black-Gray

J208-10

Upper Left
Flipper E.O.S.

 F7

	Normal          

Function Volume Up
	Test
Function
Up
	
	
	
	
	
	
	
	
	
	

	D7
	
	
	
	
	
	
	
	
	
	

	Orange-Grey
J205-9           U16-5
	8

White​-
Grey
J208-9

U19-7
	BALL
SHOOTER

18
	LEFT
WIRE

MAKE

28
	LEFT
EJECT

38
	RIGHT
CAPTIVE
BALL


48
	LEFT
CAPTIVE
BALL

58
	LOCK 3
(TOP)


68
	NOT
USED

78
	NOT
USED

88
	Black-Blue
J212-9
Upper Left
Flipper Opto

F8

	Normal          

Function  Begin Test
	Test
Function
Enter
	
	
	
	
	
	
	
	
	
	

	D8
	
	
	
	
	
	
	
	
	
	


        J2XX = CPU Board
= OPTO, TYPICALLY CLOSED
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