BRAM STOKER’S DRACULA (50001)
FUSE LIST

	POWER DRIVER BOARD
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	F101
	+50V DC General (Left Flipper)
	3A, 250V, SB Not Used
	

	F102
	+50V DC General (Right Flipper)
	3A, 250V, SB Not Used
	

	F103
	Solenoids #25 to #28
	3A, 250V, SB
	

	F104
	Solenoids #9 to #16
	3A, 250V, SB
	

	F105
	Solenoids #1 to #8
	3A, 250V, SB
	

	F106
	G.I. #5 White-Violet
	5A, 250V, SB
	

	F107
	G.I. #4 White-Green
	5A, 250V, SB
	

	F108
	G.I. #3 White-Yellow
	5A, 250V, SB
	

	F109
	G.I. #2 White-Orange
	5A, 250V, SB
	

	F110
	G.I. #1 White-Brown
	5A, 250V, SB
	

	F111
	Flasher Secondary
	5A, 250V, SB
	

	F112
	Solenoid Secondary 
	7A, 250V, SB
	

	F113
	+5V Logic
	5A, 250V, SB
	

	F114
	+18V Lamp Matrix
	8A, 32V, N.B.
	

	F115
	+12V Switch Matrix
	3/4A, 250V, FB
	

	F116
	+12V Secondary
	3A, 250V, SB
	

	Audio Board
	

	F501
	-25V Circuit
	3A, 250V, SB
	

	F502
	+25V Circuit
	3A, 250V, SB
	

	Dot Matrix Controller Board
	

	F601
	+62V Circuit
	3/8A, 250V, FB
	Fliptronic II Controller Board

	F602
	-113V & -125V Circuits
	3/8A, 250V, FB
	F901
	Upper Right Flipper
	3A, 250V, SB

	LINE FILTER
	F902
	Upper Left Flipper
	3A, 250V, SB

	Foreign
	
	5A, 250V, SB
	F903
	Lower Right Flipper
	3A, 250V, SB

	Domestic
	
	8A, 250V, SB
	F904
	Lower Left Flipper
	3A, 250V, SB


SOLENOID/FLASHER TABLE

	Sol
No.
	Function
	Solenoid
Type
	Voltage Connections
	Drive
Xistor
	Drive Connections
	Drive
Wire
Color
	Solenoid Part Number
Flashlamp Type

	
	
	
	Playfield
	Backbox
	Cabinet
	
	Playfield
	Insert
	Cabinet
	
	Playfield
	Insert

	01
	SHOOTER
	High Power
	J107-3
	
	
	Q82
	J130-1
	
	
	VIO-BRN
	AE-23-800
	

	02
	COFFIN POPPER
	High Power
	J107-3
	
	
	Q80
	J130-2
	
	
	VIO-RED
	AE-24-900
	

	03
	CASTLE POPPER
	High Power
	J107-3
	
	
	Q78
	J130-4
	
	
	VIO-ORG
	AE-26-1500
	

	04
	RIGHT RAMP DOWN
	High Power
	J107-3
	
	
	Q76
	J130-5
	
	
	VIO-YEL
	AE-26-1200
	

	05
	CRYPT POPPER
	High Power
	J107-3
	
	
	Q64
	J130-6
	
	
	VIO-GRN
	AE-25-1500
	

	06
	WIRE RAMP BALL POPPER
	High Power
	J107-3
	
	
	Q66
	J130-7
	
	
	VIO-BLU
	AE-23-800
	

	07
	KNOCKER
	High Power
	J107-3
	
	
	Q68
	J130-8
	
	
	VIO-BLK
	AE-23-800
	

	08
	SHOOTER RAMP ENTRY
	High Power
	J107-2
	
	
	Q70
	J130-9
	
	
	VIO-GRY
	AE-26-1500
	

	09
	LEFT SLINGSHOT
	Low Power
	J107-2
	
	
	Q58
	J127-1
	
	
	BRN-BLK
	AE-26-1200
	

	10
	RIGHT SLINGSHOT
	Low Power
	J107-2
	
	
	Q56
	J127-3
	
	
	BRN-RED
	AE-26-1200
	

	11
	LEFT JET BUMPER
	Low Power
	J107-2
	
	
	Q54
	J127-4
	
	
	BRN-ORG
	AE-26-1200
	

	12
	RIGHT JET BUMPER
	Low Power
	J107-2
	
	
	Q52
	J127-5
	
	
	BRN-YEL
	AE-26-1200
	

	13
	BOTTOM JET BUMPER
	Low Power
	J107-2
	
	
	Q50
	J127-6
	
	
	BRN-GRN
	AE-26-1200
	

	14
	RIGHT RAMP UP
	Low Power
	J107-2
	
	
	Q48
	J127-7
	
	
	BRN-BLU
	SM1-28-900
	

	15
	OUTHOLE
	Low Power
	J107-2
	
	
	Q46
	J127-8
	
	
	BRN-VIO
	AE-27-1200
	

	16
	TROUGH
	Low Power
	J107-2
	
	
	Q44
	J127-9
	
	
	BRN-GRY
	AE-26-1200
	

	17
	T.R. CORNER / DRACULA FL
	Flasher
	J107-6
	J106-5
	
	Q42
	J126-1
	J125-1
	
	BLK-BRN
	#906(3)
	#906(1)

	18
	JACKPOT / STOKER FLASHER
	Flasher
	J107-6
	J106-5
	
	Q40
	J126-2
	J125-2
	
	BLK-RED
	#906(1)
	#906(1)

	19
	3-BANK / HOUSE FLASHER
	Flasher
	J107-6
	J106-5
	
	Q38
	J126-3
	J125-3
	
	BLK-ORG
	#89(1)
	#906(1)

	20
	T.L CORNER / MINA FLASHER
	Flasher
	J107-6
	J106-5
	
	Q36
	J126-4
	J125-5
	
	BLK-YEL
	#89(1) #906(1)
	#906(1)

	21
	CASTLE / HELSING FLASHER
	Flasher
	J107-6
	J106-5
	
	Q28
	J126-5
	J125-6
	
	BLU-GRN
	#89(2)
	#906(1)

	22
	L. RAMP / L. LOGO FLASHER
	Flasher
	J107-6
	J106-5
	
	Q30
	J126-6
	J125-7
	
	BLU-BLK
	#906(1)
	#906(1)

	23
	R. RAMP / R. LOGO FLASHER
	Flasher
	J107-6
	J106-5
	
	Q34
	J126-7
	J125-8
	
	BLU-VIO
	#906(1)
	#906(1)

	24
	ASYLUM / RENFIELD FLASHER
	Flasher
	J107-6
	J106-5
	
	Q32
	J126-8
	J125-9
	
	BLU-GRY
	#89(1)
	#906(1)

	25
	LEFT DROP TARGET
	Low Power
	J107-1
	
	
	Q26
	*J122-1
	
	
	BLU-BRN
	AE-26-1200
	

	26
	SPEAKER PANEL FLASHER
	Low Power
	
	J106
	
	Q24
	
	J128-2
	
	BLU-RED
	
	#906(3)

	27
	MAGNET
	Low Power
	J107-1
	
	
	Q22
	*J122-3
	
	
	BLU-ORG
	20-9831
	

	28
	MAGNET’S MOTOR
	Low Power
	J107-6
	
	
	Q20
	J122-4
	
	
	BLU-YEL
	14-7981
	

	  General Illumination
	
	Voltage Connections
	Drive Xistor
	Drive Connections
	Drive
Wire
	Bulb Type

	
	
	Playfield
	Backbox
	Cabinet
	
	Playfield
	Backbox
	Cabinet
	
	Playfield
	Backbox

	01
	LOWER PLAYFIELD / INSERT
	G.I.
	J121-1
	J120-1
	
	Q18
	J121-7
	J120-7
	
	WHT-BRN
	#555
	#555

	02
	UPPER PLAYFIELD / INSERT
	G.I.
	J121-2
	J120-2
	
	Q10
	J121-8
	J120-8
	
	WHT-ORG
	#555
	#555

	03
	CENTER PLAYFIELD / INSERT
	G.I.
	J121-3
	J120-3
	
	Q14
	J121-9
	J120-9
	
	WHT-YEL
	#555
	#555

	04
	INSERT
	G.I.
	
	J120-5
	
	Q16
	
	J120-10
	
	WHT-GRN
	
	#555

	05
	INSERT
	G.I.
	
	J120-6
	J119-3
	Q12
	
	J120-11
	J119-1
	WHT-VIO
	
	#555

	  Flipper Circuits
	
	Playfield Voltage Connection
	Drive Transistors
	Playfield  Drive
	Drive Wire Colors
	Coil
Part No.
	Coil
Colors

	
	
	
	Power
	Hold
	Connections
	 Power
Hold
	
	

	
	LOWER LEFT FLIPPER
	Flipper
	J907-6, 7 (GRY-YEL)
	Q3
	Q9
	J902-7, 9
	BLU-GRY
ORG-BLU
	FL-15411
	ORANGE

	
	LOWER RIGHT FLIPPER
	Flipper
	J907-8, 9 (BLU-YEL)
	Q4
	Q11
	J902-11, 13
	BLU-VIO
ORG-GRN
	FL-15411
	ORANGE

	33
	UP / DOWN POST DIVERTER
	Up Lt. Fl. Power
	J907-2
	Q1
	
	J902-3
	BLK-BLU
	AE-26-1500
	

	34
	RIGHT GATE
	Up Lt. Fl. Hold
	J907-1
	
	Q5
	J902-1
	ORG-GRY
	AE-26-1500
	

	35
	DIS. CASTLE RELEASE POST
	Up Rt. Fl. Power
	J907-5
	Q2
	
	J902-6
	BLK-YEL
	AE-26-1500
	

	36
	LEFT BALL GATE ACTUATOR
	Up Lt. Fl. Hold
	J907-4
	
	Q7
	J902-4
	ORG-VIO
	A-14406
	


* J122-1. 3 have tieback diodes at J122-5,8 respectively.


LAMP MATRIX
Red 
Yellow (B+)
16-10213
	     Column

Row
	1

Yellow-
Brown
J137-1

Q98
	2

Yellow-
Red
J137-2

Q97
	3

Yellow-
Orange
J137-3

Q96
	4

Yellow-
Black
J137-4

Q95
	5

Yellow-
Green
J137-5

Q94
	6

Yellow-
Blue
J137-6

Q93
	7

Yellow-
Violet
J137-7

Q92
	8

Yellow-
Gray
J137-8

Q91

	1

Red-
Brown
J133-1 Q90
	NOT

USED

   11
	COFFIN

LOCK

1

21
	R. LANE:

VIDEO

“V”

  31
	RIGHT
RETURN

41
	COFFIN

LAMP

1

51
	LEFT

SKILL

100K

61
	DRACULA

“C”

71
	RATS

MODE

81

	2

Red-
Black
J133-2 Q89


	NOT
USED

12
	COFFIN

LOCK

2

22
	R. LANE:

VIDEO

“I”

32
	RIGHT

DRAIN

42
	COFFIN

LAMP

2

52
	MIDDLE

SKILL

1 MILLION

62
	DRACULA

“L”

72
	DRACULA

“A”

82

	3

Red-
Orange
J133-4 Q88


	NOT

USED

13
	DRACULA

“A”

23
	R. LANE:

VIDEO

“D”

33
	COFFIN

MULTIBALL

43
	MAGNET

53
	RIGHT

SKILL

100K

63
	LEFT

3-BANK

TOP

73
	TOP-LEFT

HOLE:

MYSTERY

83

	4

Red-
Yellow
J133-5 Q87


	NOT
USED

14
	R. RAMP:

0.5 MILLION

24
	R. LANE:

VIDEO

“E”

34
	PLAYFIELD

2X

44
	SHOOT

AGAIN

54
	TOP

3-LANE

LEFT

64
	LEFT

3-BANK

MIDDLE

74
	TOP-LEFT

HOLE:

CARRIAGE

84

	5

Red-
Green
J133-6 Q86


	NOT
USED

15
	R. RAMP:

1 MILLION

25
	R. LANE:

VIDEO

“O”

35
	CASTLE

MULTIBALL

45
	LOVE

NEVER

DIES

55
	TOP

3-LANE 

MIDDLE

65
	LEFT

3-BANK

BOTTOM

75
	TOP-LEFT

HOLE:

EXTRA BALL

85

	6

Red-
​Blue
J133-7 Q85


	R. RAMP
LOCK

16
	R. RAMP:

2.5 MILLION

26
	DRACULA

“R”

36
	PLAYFIELD

3X

46
	COFFIN

LAMP

3

56
	TOP

3-LANE

RIGHT

66
	MIDDLE

3-BANK

LEFT

76
	TOP-LEFT

HOLE:

JACKPOT

86

	7

Red​-
Violet
J133-8 Q84


	DRACULA

FACE

17
	R. RAMP:

DOUBLE

27
	LEFT

DRAIN

37
	MIST

MULTIBALL

47
	L. RAMP
ENTER

57
	DRACULA

“U”

67
	MIDDLE

3-BANK

MIDDLE

77
	LAUNCH BALL

87

	8

Red​-
Grey
J133-9 Q83


	R. RAMP:

2 MILLION

18
	R. RAMP:

1.5 MILLION

28
	LEFT

RETURN

38
	DRACULA

“D”

48
	L. RAMP

LOCK

58
	JET

INSERT

68
	MIDDLE

3-BANK

RIGHT

78
	GAME

START

88


        J1XX = Power Driver Board


SWITCH MATRIX
White
Green
	DEDICATED
GROUNDED
SWITCHES
	     Column

Row
	1

Green-
Brown
J207-1

U20-18
	2

Green-
Red
J207-2

U20-17
	3

Green-
Orange
J207-3

U20-16
	4

Green-
Yellow
J207-4

U20-15
	5

Green-
Black
J207-5

U20-14
	6

Green-
Blue
J207-6

U20-13
	7

Green-
Violet
J207-7

U20-12
	8

Green-
Grey
J207-9

U20-11
	FLIPPER
GROUNDED

SWITCHES

	Orange-Brown
J205-1
LEFT COIN
CHUTE
U17-5

D1
	1

White-
Brown
J209-1

U18-11
	NOT
USED

11
	SLAM
TILT

21
	UNDER
SHOOTER

RAMP

31
	TROUGH
1-BALL

41
	OPTO
TOP-RIGHT

LANE

51
	LEFT
JET


61
	OPTO
CASTLE

POPPER

71
	MAGNET
LEFT

81
	BLACK-GREEN
J906-1


LOWER RIGHT
E.O.S. SWITCH

F1

	Orange-Red
J205-2
CENTER COIN
CHUTE
U17-7

D2
	2

White-
Red
J209-2

U18-9
	NOT
USED


12
	COIN
DOOR
CLOSED

22
	NOT
USED


32
	TROUGH
2-BALLS


42
	OPTO
MAGNET

LEFT POCKET

52
	RIGHT
JET


62
	OPTO
COFFIN

POPPER

72
	BALL
ON

MAGNET

82
	BLUE-VIOLET
J906-2


LOWER RIGHT
FLIPPER OPTO

F2

	Orange-Black
J205-3
RIGHT COIN
CHUTE
U17-11
D3
	3

White-
Orange
J209-3

U18-5
	START
BUTTON

13
	TICKET
OPTO.

23
	NOT
USED


33
	TROUGH
3-BALLS


43
	OPTO
CASTLE 1


53
	BOTTOM
JET


63
	OPTO
LEFT RAMP

ENTRY

73
	MAGNET
RIGHT


83
	BLACK-BLUE

J906-3

LOWER LEFT
E.O.S. SWITCH

F3

	Orange-Yellow
J205-4
4TH COIN
CHUTE
U17-9

D4
	4

White-
Yellow
J209-4

U18-7
	PLUMB
BOB
TILT

14
	ALWAYS
CLOSED

24
	LAUNCH
BALL


34
	TROUGH
4-BALLS


44
	OPTO
CASTLE 2


54
	LEFT
SLING


64
	NOT
USED


74
	LEFT
RAMP
SCORE

84
	BLUE-GRAY

J905-2

LOWER LEFT
FLIPPER OPTO

F4

	Orange-Green
J205-6
	5

White-
Green
J209-5

U19-11
	LEFT
DROP
TARGET

15
	TOP
3-LANE

LEFT

25
	LEFT
DRAIN


35
	NOT
USED


45
	OPTO
WIRE RAMP
POPPER

55
	RIGHT
SLING

65
	NOT
USED


75
	LEFT
RAMP
DIVERTED


85
	BLACK-VIOLET

J906-4

UPPER RIGHT

E.O.S. SWITCH

F5

	Normal

Function

Srv Crdts
	Test

Function

Escape
	
	
	
	
	
	
	
	
	
	

	D5
	
	
	
	
	
	
	
	
	
	

	Orange-Blue
J205-7
	6

White-
​Blue
J209-7

U19-9
	LEFT
DROP
SCORE

16
	TOP
3-LANE
MIDDLE

26
	LEFT
RETURN

36
	NOT
USED


46
	OPTO
CRYPT
POPPER

56
	LEFT
3-BANK
TOP

66
	NOT
USED


76
	MIDDLE
3-BANK
LEFT


86
	BLACK-YELLOW
J905-3

UPPER RIGHT
FLIPPER OPTO

F6

	Normal

Function

Volume Dn
	Test
Function

Down
	
	
	
	
	
	
	
	
	
	

	D6
	
	
	
	
	
	
	
	
	
	

	Orange-Violet
J205-8
	7

White​-
Violet
J209-8

U19-5
	SHOOTER
LANE

17
	TOP
3-LANE

RIGHT

27
	RIGHT
RETURN 

37
	NOT

USED

47
	OPTO
CASTLE 3


57
	LEFT
3-BANK
MIDDLE

67
	RIGHT
RAMP
UP

 77
	MIDDLE
3-BANK

MIDDLE

87
	BLACK-GRAY

J906-5

UPPER LEFT
E.O.S. SWITCH

F7

	Normal

Function

Volume Up
	Test
Function
Up
	
	
	
	
	
	
	
	
	
	

	D7
	
	
	
	
	
	
	
	
	
	

	Orange-Grey
J205-9
	8

White​-
Grey
J209-9

U19-7
	NOT
USED

18
	RIGHT
RAMP

SCORE

28
	RIGHT
DRAIN


38
	OUTHOLE

48
	MYSTERY
HOLE


58
	LEFT
3-BANK
BOTTOM

68
	NOT
USED

78
	MIDDLE
3-BANK

RIGHT

88
	BLACK-BLUE
J905-5

UPPER LEFT
FLIPPER OPTO

F8

	Normal

Function

Begin Test
	Test
Function
Enter
	
	
	
	
	
	
	
	
	
	

	D8
	
	
	
	
	
	
	
	
	
	


        J2XX = CPU Board
= OPTO, TYPICALLY CLOSED



























































































































































































