	FUSE LIST
	INDIANA JONES (50017)

	POWER DRIVER BOARD
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	F101
	+50V DC General (Left Flipper)
	3A, 250V, SB
	

	F102
	+50V DC General (Right Flipper)
	3A, 250V, SB
	

	F103
	Solenoids #25 to #28
	3A, 250V, SB
	

	F104
	Solenoids #9 to #16
	3A, 250V, SB
	

	F105
	Solenoids #1 to #8
	3A, 250V, SB
	

	F106
	G.I. #5 White-Violet
	5A, 250V, SB
	

	F107
	G.I. #4 White-Green
	5A, 250V, SB
	

	F108
	G.I. #3 White-Yellow
	5A, 250V, SB
	

	F109
	G.I. #2 White-Orange
	5A, 250V, SB
	

	F110
	G.I. #1 White-Brown
	5A, 250V, SB
	

	F111
	Flasher Secondary
	5A, 250V, SB
	

	F112
	Solenoid Secondary 
	7A, 250V, SB
	

	F113
	+5V Logic
	5A, 250V, SB
	

	F114
	+18V Lamp Matrix
	8A, 32V, N.B.
	

	F115
	+12V Lamp Matrix
	3/4A, 250V, FB
	

	F116
	+12V Secondary
	3A, 250V, SB
	

	Audio Board
	

	F501
	-25V
	3A, 250V, SB
	

	F502
	+25V
	3A, 250V, SB
	

	Dot Matrix Controller Board
	

	F601
	+62V
	3/8A, 250V, FB
	Fliptronic II Controller Board

	F602
	-113V & -125V
	3/8A, 250V, FB
	F901
	Upper Right Flipper
	3A, 250V, SB

	LINE FILTER
	F902
	Upper Left Flipper
	3A, 250V, SB

	Foreign
	
	5A, 250V, SB
	F903
	Lower Right Flipper
	3A, 250V, SB

	Domestic
	
	8A, 250V, SB
	F904
	Lower Left Flipper
	3A, 250V, SB


SOLENOID/FLASHER TABLE

	Sol
No.
	Function
	Solenoid
Type
	Voltage Connections
	Drive
Xistor
	Drive Connections     
	Drive Wire
Color
	Coil/Flashlamp Type

	
	
	
	Playfield
	Backbox
	Cabinet
	
	Playfield
	Insert
	Cabinet
	
	Playfield
	Insert

	01
	BALL POPPER
	High Power
	J107-3
	
	
	Q82
	J130-1
	
	
	VIO-BRN
	AE-26-1200
	

	02
	BALL LAUNCH
	High Power
	J107-3
	
	
	Q80
	J130-2
	
	
	VIO-RED
	AE-23-800
	

	03
	TOTEM DROP UP
	High Power
	J107-3
	
	
	Q78
	J130-4
	
	
	VIO-ORG
	AE-26-1200
	

	04
	BALL RELEASE
	High Power
	J107-3
	
	
	Q76
	J130-5
	
	
	VIO-YEL
	AE-26-1500
	

	05
	CENTER DROP BANK
	High Power
	J107-3
	
	
	Q64
	J130-6
	
	
	VIO-GRN
	AE-26-1200
	

	06
	IDOL RELEASE
	High Power
	J107-3
	
	
	Q66
	J130-7
	
	
	VIO-BLU
	AE-26-1500
	

	07
	KNOCKER
	High Power
	J107-3
	
	
	Q68
	J130-8
	
	
	VIO-BLK
	AE-23-800
	

	08
	LEFT EJECT
	High Power
	J107-3
	
	
	Q70
	J130-9
	
	
	VIO-GRY
	AE-26-1200
	

	09
	LEFT JET BUMPER
	Low Power
	J107-2
	
	
	Q58
	J127-1
	
	
	BRN-BLK
	AE-26-1200
	

	10
	RIGHT JET BUMPER
	Low Power
	J107-2
	
	
	Q56
	J127-3
	
	
	BRN-RED
	AE-26-1200
	

	11
	BOTTOM JET BUMPER
	Low Power
	J107-2
	
	
	Q54
	J127-4
	
	
	BRN-ORG
	AE-26-1200
	

	12
	LEFT SLINGSHOT
	Low Power
	J107-2
	
	
	Q52
	J127-5
	
	
	BRN-YEL
	AE-27-1200
	

	13
	RIGHT SLINGSHOT
	Low Power
	J107-2
	
	
	Q50
	J127-6
	
	
	BRN-GRN
	AE-27-1200
	

	14
	LEFT CONTROL GATE
	Low Power
	J107-2
	
	
	Q48
	J127-7
	
	
	BRN-BLU
	A-14406
	

	15
	RIGHT CONTROL GATE
	Low Power
	J107-2
	
	
	Q46
	J127-8
	
	
	BRN-VIO
	A-14406
	

	16
	TOTEM DROP DOWN
	Low Power
	J107-2
	
	
	Q44
	J127-9
	
	
	BRN-GRY
	SM1-26-600
	

	17
	ETERNAL LIFE
	Flasher
	J107-6
	J106-5
	
	Q42
	J126-1
	J125-1
	
	BLK-BRN
	#906
	#906 (3)

	18
	LIGHT JACKPOT
	Flasher
	J107-6
	
	
	Q40
	J126-2
	
	
	BLK-RED
	#906
	

	19
	SUPER JACKPOT
	Flasher
	J107-6
	
	
	Q38
	J126-3
	
	
	BLK-ORG
	#89
	

	20
	JACKPOT
	Flasher
	J107-6
	J106-5
	
	Q36
	J126-4
	J125-5
	
	BLK-YEL
	#89
	#906 (2)

	21
	PATH OF ADVENTURE
	Flasher
	J107-6
	J106-5
	
	Q28
	J126-5
	J125-6
	
	BLU-GRN
	#89
	#906 (4)

	22
	MINI MOTOR LEFT
	Low Power
	J118-2
	
	
	Q30
	J126-6
	
	
	BLU-BLK
	
	

	23
	MINI MOTOR RIGHT
	Low Power
	J118-2
	
	
	Q34
	J126-7
	
	
	BLU-VIO
	14-7988
	

	24
	PLANE GUN LEDS
	Flasher
	J118-2
	J106-5
	
	Q32
	J126-8
	
	
	BLU-GRY
	A-16834
	

	25
	DOGFIGHT HURRY UP
	Gen. Purpose
	J107-6
	
	
	Q26
	J122-1
	
	
	BLU-BRN
	#89
	

	26
	RIGHT RAMP
	Gen. Purpose
	J107-6
	J106-5
	
	Q24
	J122-2
	J124-2
	
	BLU-RED
	#89 (3)
	#906

	27
	LEFT RAMP
	Gen. Purpose
	J107-6
	J106-5
	
	Q22
	J122-3
	J124-3
	
	BLU-ORG
	#89
	#906

	28
	SUBWAY RELEASE
	Gen. Purpose
	J107-1
	
	
	Q20
	J122-4
	
	
	BLU-YEL
	AE-26-1500
	

	37
	LEFT SIDE FLASHER
	Low Power
	J107-6
	J106-5
	
	Q16
	* J4-2
	J4-2
	
	BRN-WHT
	#89 (2)
	#906

	38
	RIGHT SIDE FLASHER
	Low Power
	J107-6
	J106-5
	
	Q15
	* J4-4
	J4-4
	
	BLK-WHT
	#89 (2)
	#906

	39
	SPECIAL FLASHER
	Low Power
	J107-6
	
	
	Q14
	* J4-5
	
	
	ORG-WHT
	#89 (2)
	

	40
	TOTEM MULTIBALL
	Low Power
	J107-6
	
	
	Q13
	* J4-6
	
	
	YEL-WHT
	#89
	

	41
	JACKPOT MULTIPLIER FLSH
	Low Power
	J107-6
	
	
	Q9
	* J3-2
	
	
	GRN-WHT
	#89
	

	42
	WHEEL MOTOR
	Low Power
	J118-2
	
	
	Q10
	* J3-3
	
	
	BLU-WHT
	14-7982
	

	  General Illumination
	
	Voltage Connections
	Drive Xistor
	Drive Connections
	Drive
Wire
	Bulb Type

	
	
	Playfield
	Insert
	Cabinet
	
	Playfield
	Insert
	Cabinet
	
	Playfield
	Insert

	01
	TOP PLAYFIELD
	G.I.
	J121-1
	
	
	Q18
	J121-7
	
	
	WHT-BRN
	#44
	

	02
	BOTTOM PLAYFIELD
	G.I.
	J121-2
	
	
	Q10
	J121-8
	
	
	WHT-ORG
	#44
	

	03
	INSERT TOP
	G.I.
	
	J120-3
	
	Q14
	
	J120-9
	
	WHT-YEL
	
	#555

	04
	INSERT BOTTOM
	G.I.
	
	J120-4
	
	Q16
	
	J120-10
	
	WHT-GRN
	
	#555

	05
	RETURN LANE / COIN
	G.I.
	J121-6
	
	J119-3
	Q12
	J121-11
	
	J119-1
	WHT-VIO
	#44
	

	  Flipper Circuits
	
	Playfield Voltage Connection
	Drive Transistors
	Playfield  Drive
	Drive Wire Colors
	Coil
Part No.
	Coil
Colors

	
	
	
	Power
	Hold
	Connections
	 Power            Hold
	
	

	29
	LOWER RIGHT FLIPPER
	Power
	J907-9 (BLU-YEL)
	Q4
	
	J902-13
	BLU-VIO
	FL-11629
	BLUE

	30
	
	Hold
	J907-9 (BLU-YEL)
	
	Q11
	J902-11
	ORG-GRN
	
	

	31
	LOWER LEFT FLIPPER
	Power
	J907-7 (GRY-YEL)
	Q3
	
	J902-9
	BLU-GRY
	FL-11629
	BLUE

	32
	
	Hold
	J907-7 (GRY-YEL)
	
	Q9
	J902-7
	ORG-BLU
	
	

	33
	DIVERTER
	Power
	J907-1 (BLU-YEL)
	Q2
	
	J902-6
	BLK-YEL
	FL-11753-1
	YELLOW

	34
	
	Hold
	J907-1 (BLU-YEL)
	
	Q7
	J902-4
	ORG-VIO
	
	

	35
	TOP LOCKUP
	Power
	J907-4 (GRY-YEL)
	Q1
	
	J902-3
	BLK-BLU
	A-15943
	BROWN

	36
	
	Hold
	J907-4 (GRY-YEL)
	
	Q5
	J902-1
	ORG-GRY
	
	

	* From 8 Driver PCB, A-16100


	** From D.C. Motor Control Assembly, A-16120

	





	
LAMP MATRIX
	
	
	Yellow (B+)
	[image: image2.wmf]
	  Red

	      Column

Row
	1

Yellow-
Brown
J137-1

Q98
	2

Yellow-
Red
J137-2

Q97
	3

Yellow-
Orange
J137-3

Q96
	4

Yellow-
Black
J137-4

Q95
	5

Yellow-
Green
J137-5

Q94
	6

Yellow-
Blue
J137-6

Q93
	7

Yellow-
Violet
J137-7

Q92
	8

Yellow-
Grey
J137-9

Q91

	1

Red-
Brown
J133-1 Q90
	MODE 

START

   11
	TANK

CHASE

21
	LEFT
RAMP

ARROW

  31
	MINE

CART

41
	CHOOSE 

WISELY

51
	(I)NDY

61
	MINI

TOP

LEFT

71
	MINI

MIDDLE

BOTTOM

LEFT

81

	2

Red-
Black
J133-2 Q89
	HAND OF

FATE


12
	ADVEN(T)URE

LIGHT

22
	CASTLE

GRUNEWALD

32
	ARK

JACKPOT

42
	RIGHT

PLANE

TOP

52
	I(N)DY

62
	MINI

TOP

RIGHT

72
	MINI

MIDDLE

BOTTOM

RIGHT

82

	3

Red-
Orange
J133-4 Q88


	EJECT

EXTRA

BALL

13
	ADV(E)NTURE

LIGHT

23
	LEFT

PLANE

TOP

33
	RAVEN
BAR


43
	ROPE

BRIDGE

53
	
IN(D)Y

63
	MINI

MIDDLE
TOP LEFT

73
	MINI

BOTTOM

LEFT

83

	4

Red-
Yellow
J133-5 Q87


	AD(V)ENTURE

LIGHT

14
	ADVE(N)TURE
LIGHT


24
	MONKEY

BRAINS


34
	RIGHT
PLANE

MIDDLE

44
	ADVENT(U)RE

LIGHT

54
	IND(Y)

64
	MINI

MIDDLE

TOP RIGHT

74
	MINI

BOTTOM

RIGHT

84

	5

Red-
Green
J133-6 Q86


	A(D)VENTURE
LIGHT

15
	STEAL
THE STONES

25
	LEFT

PLANE

MIDDLE

35
	BONUS

6 X

45
	ADVENTU(R)E
​LIGHT

55
	WILLIE

65
	MINI

ARROW

TOP

75
	MINI

BOTTOM

ARROW

85

	6

Red-
​Blue
J133-7 Q85


	(A)DVENTURE
LIGHT

16
	GRAIL
JACKPOT

26
	SALLAH


36
	RIGHT

PLANE

BOTTOM

46
	ADVENTUR(E)

LIGHT

56
	BONUS

2 X

66
	MARION

76
	TOTEM TOP
ARROW

86

	7

Red​-
Violet
J133-8 Q84


	SHOOT

AGAIN

17
	STREETS

OF

CAIRO

27
	BONUS
4 X

37
	WELL
OF

SOULS

47
	THE
3
CHALLENGES

57
	SHORTY

67
	BONUS
8 X

77
	CENTER

LOCK

87

	8

Red​-
Grey
J133-9 Q83


	GET

THE

IDOL

18
	STONES

JACKPOT

28
	LEFT

PLANE

BOTTOM

38
	LEFT

LOOP

48
	RIGHT
LOOP


58
	RIGHT

RAMP

ARROW

68
	DR.

JONES

78
	START 

BUTTON

88


        J1XX = Power Driver Board

	SWITCH MATRIX
	
	
	Green
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	 White
	

	DEDICATED
GROUNDED
SWITCHES
	   Column

Row
	1

Green-
Brown
J207-1

U20-18
	2

Green-
Red
J207-2

U20-17
	3

Green-
Orange
j207-3

U20-16
	4

Green-
Yellow
j207-4

U20-15
	5

Green-
Black
j207-5

U20-14
	6

Green-
Blue
J207-6

U20-13
	7

Green-
Violet
J207-7

U20-12
	8

Green-
Grey
J207-9

U20-11
	9

Grey-

White
*J5-4

Q11
	FLIPPER
GROUNDED

SWITCHES

	Orange-Brown
J205-1
LEFT COIN
CHUTE


D1
	 1

White-
Brown
J209-1

U18-11
	SINGLE
DROP

TARGET

  11
	SLAM
TILT

21
	LEFT
EJECT

  31
	LEFT

RAMP

ENTER

41
	ADVENT-
(U)RE

TARGET

51
	(A)DVENT-
URE

TARGET

61
	CAPTIVE
BALL

FRONT

71
	TROUGH
6

81
	WHEEL

POSITION

1

91
	Black-Green
J906-1

Lower Right
Flipper E.O.S.

F1

	Orange-Red
J205-2
CENTER COIN
CHUTE


D2
	 2

White-
Red
J209-2

U18-9
	BUY-IN
BUTTON


12
	COIN
DOOR
CLOSED

22
	EXIT
IDOL


32
	RIGHT
RAMP
ENTER

42
	ADVENT-
U(R)E

TARGET

52
	A(D)VENT-
URE

TARGET

62
	MINI
TOP

HOLE

72
	TROUGH
5

82
	WHEEL

POSITION

2

92
	Black-Violet
J905-1
Lower Right
Flipper Opto
F2

	Orange-Black
J205-3
RIGHT COIN
CHUTE

D3
	 3

White-
Orange
J209-3

U18-5
	START
BUTTON

13
	TICKET
OPTO

23
	LEFT

SLINGSHOT


33
	TOP
IDOL

ENTER

43
	ADVENT-

UR(E)
TARGET

53
	AD(V)ENT-
URE
TARGET

63
	MINI
BOTTOM

HOLD

73
	TROUGH
4

83
	WHEEL

POSITION

3

93
	Black-Blue

J906-3

Lower Left
Flipper E.O.S.

F3

	Orange-Yellow
J205-4
4TH COIN
CHUTE


D4
	 4

White-
Yellow
J209-4

U18-7
	PLUMB
BOB
TILT

14
	ALWAYS
CLOSED

24
	GUN
TRIGGER

34
	RIGHT

POPPER


44
	LEFT
LOOP
TOP

54
	CAPTIVE
BALL
BACK

64
	RIGHT

RAMP
MADE

74
	TROUGH
3

84
	MINI

PLAYFIELD

LEFT

LIMIT

94
	Black-Gray

J905-2

Lower Left
Flipper Opto

F4

	Orange-Green
J205-6         
	 5

White-
Green
J209-5

U19-11
	LEFT
OUTLANE


15
	(I)NDY
LANE

25
	LEFT
JET


35
	CENTER

ENTER


45
	LEFT
LOOP
BOTTOM

55
	MINI
TOP

LEFT

65
	MINI
TOP
RIGHT

75
	TROUGH
2

85
	MINI

PLAYFIELD

RIGHT

LIMIT

95
	Black-Violet

J906-4

Upper Right

Flipper E.O.S.

F5

	Normal  
Function
Srv Crdts
	Test Function

Escape
	
	
	
	
	
	
	
	
	
	
	

	D5
	
	
	
	
	
	
	
	
	
	
	

	Orange-Blue
J205-7          
	 6

White-
​Blue
J209-7

U19-9
	LEFT
RETURN
LANE

16
	I(N)DY
LANE

26
	RIGHT
JET

36
	TOP
POST


46
	RIGHT
LOOP
TOP

56
	MINI
MIDDLE
TOP

LEFT

66
	MINI
MIDDLE
TOP

RIGHT

76
	TROUGH
1

86
	
	Black-Yellow
J905-3

Upper Right
Flipper Opto

F6

	Normal          

Function Volume Dn
	Test
Function

Down
	
	
	
	
	
	
	
	
	
	
	

	D6
	
	
	
	
	
	
	
	
	
	
	

	Orange-Violet
J205-8          
	 7

White​-
Violet
J209-8

U19-5
	RIGHT
RETURN
LANE

17
	IN(D)Y
LANE

27
	BOTTOM

JET

37
	SUBWAY
LOCKUP

47
	RIGHT

LOOP

BOTTOM

57
	MINI
MIDDLE
BOTTOM

LEFT

67
	MINI
MIDDLE
BOTTOM

RIGHT

 77
	TOP
TROUGH

87
	
	Black-Gray

J906-5

Upper Left
Flipper E.O.S.

 F7

	Normal          

Function Volume Up
	Test
Function
Up
	
	
	
	
	
	
	
	
	
	
	

	D7
	
	
	
	
	
	
	
	
	
	
	

	Orange-Grey
J205-9           
	 8

White​-
Grey
J209-9

U19-7
	RIGHT
OUTLANE

TOP

18
	IND(Y)
LANE

28
	CENTER
STANDUP

38
	RIGHT
SLINGSHOT



48
	RIGHT
OUTLANE

BOTTOM

58
	MINI
BOTTOM
LEFT

68
	MINI
BOTTOM

RIGHT

78
	SHOOTER


88
	
	Black-Blue
J905-5
Upper Left
Flipper Opto

F8

	Normal          

Function  Begin Test
	Test
Function
Enter
	
	
	
	
	
	
	
	
	
	
	

	D8
	
	
	
	
	
	
	
	
	
	
	

	J2XX = CPU Board;  J9XX = Fliptronic II Board;
	
	
	  = OPTO, TYPICALLY CLOSED
	*Located on 8 driver PCB, A-16100, in backbox




























































































































































































