NO GOOD GOFERS (50061)
                                      
FUSE LIST
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	F101
	Regulated 12V
	T0.63A, 250V
	
	

	F102
	Solenoids #9 to #16
	T4.0A, 250V
	
	

	F103
	Solenoids #1 to #8
	T4.0A, 250V
	
	

	F104
	Solenoids #25 to #28
	T4.0A, 250V
	
	

	F105
	+5V Logic
	T4.0A, 250V
	
	

	F106
	+18V Lamp Matrix
	T5.0A, 250V
	
	

	F107
	Flasher Secondary
	T4.0A, 250V
	
	

	F108
	Solenoid Secondary
	T6.3A, 250V
	
	

	F109
	Unregulated 12V
	T4.0A, 250V
	
	

	F110
	G.I. #5 White-Violet
	T4.0A, 250V
	CAUTION: FOR CONTINUED PROTECTION AGAINST RISK OF FIRE, REPLACE ONLY WITH THE SAME TYPE OF FUSE HAVING THE SAME ELECTRICAL RATINGS.
	

	F111
	G.I. #4 White-Green
	T4.0A, 250V
	
	

	F112
	G.I. #3 White-Yellow
	T4.0A, 250V
	
	

	F113
	G.I. #2 White-Orange
	T4.0A, 250V
	
	

	F114
	G.I. #1 White-Brown
	T4.0A, 250V
	AUDIO/VIDEO BOARD
	

	F115
	+50V Flippers
	T4.0A, 250V
	F501
	-25V
	T2.5A, 250V
	

	F116
	+50V Flippers
	T4.0A, 250V
	F502
	+25V
	T2.5A, 250V
	LINE FILTER

	F117
	+50V Flippers
	T4.0A, 250V
	F601
	+62V
	T0.25A, 250V
	Foreign
	T4.0A, 250V

	F118
	+50V Flippers
	T4.0A, 250V
	F602
	-113V & -125V
	T0.25A, 250V
	Domestic
	T5.0A, 250V


SOLENOID/FLASHER TABLE

	Sol
No.
	Function
	Solenoid
Type
	Voltage Connections
	Drive
Xistor
	Drive Connections     
	Drive Wire
Color
	Solenoid/Flashlamp

	
	
	
	Playfield
	Backbox
	Cabinet
	
	Playfield
	Backbox
	Cabinet
	
	Playfield
	Backbox

	01
	AUTO FIRE
	High Power
	J133-2
	
	
	Q72
	J116-1
	
	
	VIO-BRN
	AE-23-800
	

	02
	KICKBACK
	High Power
	
	J134-3
	
	Q68
	J116-2
	
	
	VIO-RED
	AE-23-800
	

	03
	CLUBHOUSE KICKER
	High Power
	J133-2
	
	
	Q71
	J116-4
	
	
	VIO-ORG
	AE-23-800
	

	04
	LEFT GOFER UP
	High Power
	J133-2
	
	
	Q67
	J116-5
	
	
	VIO-YEL
	LE-22-925
	

	05
	RIGHT GOFER UP
	High Power
	J133-2
	
	
	Q70
	J116-6
	
	
	VIO-GRN
	LE-22-925
	

	06
	JET POPPER
	High Power
	J133-2
	
	
	Q66
	J116-7
	
	
	VIO-BLU
	AE-27-1200
	

	07
	LEFT EJECT
	High Power
	J133-2
	
	
	Q69
	J116-8
	
	
	VIO-BLK
	AE-24-900
	

	08
	UPPER RIGHT EJECT
	High Power
	J133-2
	
	
	Q65
	J116-9
	
	
	VIO-GRY
	AE-27-1200
	

	09
	TROUGH EJECT
	Low Power
	J133-3
	
	
	Q44
	J113-1
	
	
	BRN-BLK
	AE-26-1500
	

	10
	LEFT SLINGSHOT
	Low Power
	J133-3
	
	
	Q48
	J113-3
	
	
	BRN-RED
	AE-27-1200
	

	11
	RIGHT SLINGSHOT
	Low Power
	J133-3
	
	
	Q43
	J113-4
	
	
	BRN-ORG
	AE-27-1200
	

	12
	TOP JET BUMPBER
	Low Power
	J133-3
	
	
	Q47
	J113-5
	
	
	BRN-YEL
	AE-26-1200
	

	13
	MIDDLE JET BUMPER
	Low Power
	J133-3
	
	
	Q42
	J113-6
	
	
	BRN-GRN
	AE-26-1200
	

	14
	BOTTOM JET BUMPER
	Low Power
	J133-3
	
	
	Q46
	J113-7
	
	
	BRN-BLU
	AE-26-1200
	

	15
	LEFT GOFER DOWN
	Low Power
	J133-3
	
	
	Q41
	J113-8
	
	
	BRN-VIO
	AE-30-2000
	

	16
	RIGHT GOFER DOWN
	Low Power
	J133-3
	
	
	Q45
	J114-9
	
	
	BRN-GRY
	AE-30-2000
	

	17
	JET FLASHER
	Flasher
	J133-6
	
	
	Q28
	J111-1
	
	
	BLK-BRN
	#906
	

	18
	LOWER LEFT FLASHER
	Flasher
	J133-6
	
	
	Q32
	J111-2
	
	
	BLK-RED
	#906
	

	19
	LEFT SPINNER FLASHER
	Flasher
	J133-6
	
	
	Q27
	J111-3
	
	
	BLK-ORG
	#906
	

	20
	RIGHT SPINNER FLASHER
	Flasher
	J133-6
	
	
	Q31
	J111-4
	
	
	BLK-YEL
	#906, #89
	

	21
	LOWER RIGHT FLASHER
	Flasher
	J133-2
	
	
	Q26
	J111-5
	
	
	BLU-GRN
	#89
	

	22
	NOT USED
	Flasher
	
	
	
	Q30
	
	
	
	BLU-BLK
	
	

	23
	NOT USED
	Flasher
	
	
	
	Q25
	
	
	
	BLU-VIO
	
	

	24
	UNDERGROUND PASS
	Flasher
	J133-1
	
	
	Q29
	J111-8
	
	
	BLU-GRY
	AE-27-1200
	

	25
	SAND TRAP FLASHER
	Gen. Purpose
	J133-6
	
	
	Q16
	J109-1
	
	
	BLU-BRN
	#906 (2)
	

	26
	WHEEL FLASHER
	Gen. Purpose
	J133-6
	
	
	Q15
	J109-2
	
	
	BLU-RED
	#906
	

	27
	LEFT RAMP DOWN
	Gen. Purpose
	J133-1
	
	
	Q14
	J109-3
	
	
	BLU-ORG
	SM1-28-900
	

	28
	RIGHT RAMP DOWN
	Gen. Purpose
	J133-1
	
	
	Q13
	J109-4
	
	
	BLU-YEL
	SM1-28-900
	

	  General Illumination
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	01
	LEFT SIDE STRING
	G.I.
	J105-1
	
	
	Q5
	J105-7
	
	
	WHT-BRN
	
	#555, #545

	02
	RIGHT SIDE STRING
	G.I.
	J105-2
	
	
	Q4
	J105-8
	
	
	WHT-ORG
	
	#555, #545

	03
	GOFER SPOTLIGHT
	G.I.
	J105-3
	
	
	Q3
	J105-9
	
	
	WHT-YEL
	#44
	#555

	04
	*ILLUMINATION STRING 4
	G.I.
	
	J106-5
	
	Q2
	
	J106-10
	
	WHT-GRN
	#44
	

	05
	*ILLUMINATION STRING 5
	G.I.
	
	J106-6
	J104-3
	Q1
	
	J106-11
	J104-1
	WHT-VIO
	#44
	

	  Flipper Circuits
	
	Voltage Connection

Playfield
	Drive Xistors
	Drive Connections
	Drive Wire Colors
	Coil
Part No.
	Coil
Colors

	
	
	
	Power
	Hold
	Playfield
	Power                Hold
	
	

	29
	LOWER RIGHT FLIPPER
	Power
	J119-1 (RED-GRN)
	Q90
	
	J120-13
	YEL-GRN
	FL-11629
	BLUE

	30
	
	Hold
	J119-1 (RED-GRN)
	
	Q92
	J120-11
	ORG-GRN
	
	

	31
	LOWER LEFT FLIPPER
	Power
	J119-4 (RED-BLU)
	Q67
	
	J120-9
	YEL-BLU
	FL-11629
	BLUE

	32
	
	Hold
	J119-4 (RED-BLU)
	
	Q69
	J120-7
	ORG-BLU
	
	

	33
	UPPER RIGHT FLIPPER
	Power
	J119-6 (RED-VIO)
	Q84
	
	J120-6
	YEL-VIO
	  FL-11630
	RED

	34
	
	Hold
	J119-6 (RED-VIO
	
	Q86
	J120-4
	ORG-VIO
	
	

	35
	BALL LAUNCH RAMP
	Power
	J119-8 (RED-GRY)
	Q81
	
	J120-3
	YEL-GRY
	  B-13522
	YELLOW

	36
	NOT USED
	Hold
	J119-8 (RED-GRY)
	
	Q83
	J120-1
	ORG-GRY
	
	

	  Motor Circuit
	Solenoid Type
	Voltage Connection

Playfield
	Drive Gates
	Drive Connections Playfield
	Drive Wire Color
	Device Part Number

Playfield

	37
	WHEEL SPIN (CCW)
	Low Power
	J139-2
	U3A
	U3B
	J110-1
	BRN-WHT
	SEE 
	MANUAL

	38
	WHEEL SPIN (CLOCK-WISE)
	Low Power
	J139-2
	U3C
	U3D
	J110-3
	ORG-WHT
	SEE
	MANUAL

	  Auxiliary Circuit
	Solenoid Type
	Voltage Connection

Playfield
	Drive Gates
	Drive Connections Playfield
	Drive Wire Color
	Device Part Number

Playfield

	42
	UPPER RIGHT 1 FLASHER
	Flasher
	J4-1
	Q2
	
	J4-2
	BLU-BRN
	#906
	

	43
	UPPER RIGHT 2 FLASHER
	Flasher
	J4-1
	Q4
	
	J4-3
	BLU-RED
	#906
	

	44
	UPPER RIGHT 3 FLASHER
	Flasher
	J4-1
	Q6
	
	J4-4
	BLU-ORG
	#906
	

	45
	UPPER PLAYFIELD RIGHT
	Flasher
	J4-1
	Q8
	
	J4-5
	BLU-ORG
	#906 (2)
	

	46
	UPPER PLAYFIELD LEFT
	Flasher
	J4-1
	Q10
	
	J4-7
	BLU-GRN
	#906
	

	47
	UPPER LEFT 1 FLASHER
	Flasher
	J4-1
	Q12
	
	J4-8
	BLU-BLK
	#906
	

	48
	UPPER LEFT 2 FLASHER
	Flasher
	J4-1
	Q14
	
	J4-9
	BLU-VIO
	#906
	

	49
	UPPER LEFT 3 FLASHER
	Flasher
	J4-1
	Q16
	
	J4-10
	BLU-GRY
	#906
	





      LAMP MATRIX
Yellow (B+)    
Red
16-10531
	     Column

 Row
	1

Yellow-
Brown
J121-1

Q96
	2

Yellow-
Red
J121-2

Q100
	3

Yellow-
Orange
J121-3

Q95
	4

Yellow-
Black
J121-4

Q99
	5

Yellow-
Green
J121-5

Q94
	6

Yellow-
Blue
J121-6

Q98
	7

Yellow-
Violet
J121-7

Q93
	8

Yellow-
Grey
J121-8

Q97

	1

Red-
Brown
J125-1 Q104
	OUTLANE 

EXTRA

BALL

   11
	HOLE

5

21
	HOLE
6

  31
	DRIVING

RANGE

41
	(K)ICK

51
	4

STROKES

61
	ADVANCE

TRAP

71
	SIDE

RAMP

DRIVE

81

	2

Red-
Black
J125-2 Q108
	KICKBACK 

12
	HOLE

4

22
	HOLE

7

32
	INCREASE

GOLF 

CART

42
	K(I)CK

52
	3

STROKES

62
	CENTER

DRIVE

72
	EXTRA

BALL

82

	3

Red-
Orange
J125-4 Q103


	LOWER
DRIVING

RANGE

13
	HOLE

3

23
	HOLE

2

33
	INCREASE
BUZZ
VALUE

43
	KIC(C)K

53
	2
STROKES

63
	CENTER
LOCK

73
	MULTIBALL

83

	4

Red-
Yellow
J125-5 Q107


	SHOOT
​AGAIN

14
	HIT BUD



24
	HIT BUZZ

34
	INCREASE
BUD

VALUE

44
	KIC(K)

54
	5

STROKES

64
	GET

T.N.T.

74
	JACKPOT

84

	5

Red-
Green
J125-6 Q102


	SPECIAL


15
	HOLE
1

25
	HOLE

9

35
	NEWTON 

DRIVE

45
	SKILL
​SHOT

55
	7

STROKES

65
	CENTER

RAISE

GOFER

75
	PUTT

OUT

85

	6

Red-
​Blue
J125-7 Q106


	WHEEL
VALUE

16
	2X


26
	4X


36
	COLLECT

46
	RIGHT

RAISE

GOFER

56
	6

STROKES

66
	RIGHT

SPINNER

76
	TOP
JET

BUMPER

86

	7

Red​-
Violet
J125-8 Q101


	JET

LIGHTNING

17
	CART PATH

2

27
	CART PATH
4

37
	RIP OFF


47
	RIGHT
RAMP
LOCK

57
	LEFT

SPINNER

67
	RIGHT
LOOP

DRIVE

77
	MIDDLE

JET

BUMPER

87

	8

Red​-
Grey
J125-9 Q105


	HOLE

8

18
	5X

CART PATH 

28
	3X 

38
	LEFT 

LOOP

DRIVE

48
	RIGHT
RAMP
DRIVE

58
	TRAP

READY

68
	BOTTOM

JET

BUMPER

78
	START BUTTON

88


        J1XX = Power Driver Board

SWITCH MATRIX
White
Green
	DEDICATED
GROUNDED
SWITCHES
	    Column

Row
	1

Green-
Brown
J206-1

U20-18
	2

Green-
Red
J206-2

U20-17
	3

Green-
Orange
J206-3

U20-16
	4

Green-
Yellow
J206-4

U20-15
	5

Green-
Black
J206-5

U20-14
	6

Green-
Blue
J206-6

U20-13
	7

Green-
Violet
J206-7

U20-12
	8

Green-
Grey
J206-9

U20-11
	FLIPPER
GROUNDED

SWITCHES

	Orange-Brown
J205-1
LEFT COIN
CHUTE
U17-5

D1
	1

White-
Brown
J208-1

U18-11
	NOT
USED

  11
	SLAM
TILT

21
	TROUGH
EJECT

  31
	LEFT
GOFER

DOWN

41
	LEFT
SLING

51
	LEFT
SPINNER


61
	LEFT
CART

PATH

71
	K-I-C-K
ADVANCE

81
	Black-Green
J208-13
Lower Right
Flipper E.O.S.

F1

	Orange-Red
J205-2
CENTER COIN
CHUTE
U17-7

D2
	2

White-
Red
J208-2

U18-9
	LEFT
RAMP
MAKE

12
	COIN
DOOR
CLOSED

22
	TROUGH
BALL
1

32
	RIGHT
GOFER
DOWN

42
	RIGHT
SLING

52
	RIGHT
SPINNER

62
	RIGHT
CART

PATH

72
	(K)ICK


82
	Blue-Violet
J212-12
Lower Right
Flipper Opto

F2

	Orange-Black
J205-3
RIGHT COIN
CHUTE
U17-11
D3
	3

White-
Orange
J208-3

U18-5
	START
BUTTON

13
	JET
ADVANCE

STANDUP

23
	TROUGH
BALL
2

33
	NOT
USED

43
	TOP
JET
BUMPER

53
	INNER
WHEEL
OPTO

63
	RIGHT
RAMP

MAKE

73
	K(I)CK


83
	Black-Blue

J208-12

Lower Left
Flipper E.O.S.

F3

	Orange-Yellow
J205-4
4TH COIN
CHUTE
U17-9

D4
	4

White-
Yellow
J208-4

U18-7
	PLUMB
BOB
TILT

14
	ALWAYS
CLOSED

24
	TROUGH
BALL
3

34
	PUTT
OUT
POPPER

44
	MIDDLE
JET
BUMPER

54
	OUTER
WHEEL
OPTO

64
	GOLF
CART


74
	KI(C)K


84
	Blue-Gray

J212-11

Lower Left
Flipper Opto

F4

	Orange-Green
J205-6         U16-9
	5

White-
Green
J208-5

U19-11
	CENTER
RAMP
MAKE

15
	UNDER-
GROUND

PASS

25
	TROUGH
BALL
4

35
	RIGHT
POPPER
JAM

45
	BOTTOM
JET
BUMPER

55
	LEFT
GOFER

1

65
	RIGHT
GOFER
1

75
	KIC(K)


85
	Black-Violet

J208-11

Upper Right

Flipper E.O.S.

F5

	Normal  
Function
Srv Crdts
	Test Function

Escape
	
	
	
	
	
	
	
	
	
	

	D5
	
	
	
	
	
	
	
	
	
	

	Orange-Blue
J205-7          U16-11
	6

White-
​Blue
J208-7

U19-9
	LEFT
OUTLANE


16
	LEFT
IN-LANE

26
	TROUGH
BALL

5

36
	RIGHT
POPPER


46
	TOP
SKILL
SHOT

56
	LEFT
GOFER
2

66
	RIGHT
GOFER
2

76
	CAPTIVE
BALL

86
	Black-Yellow
J212-10
Upper Right
Flipper Opto

F6

	Normal          

Function Volume Dn
	Test
Function

Down
	
	
	
	
	
	
	
	
	
	

	D6
	
	
	
	
	
	
	
	
	
	

	Orange-Violet
J205-8          U16-7
	7

White​-
Violet
J208-8

U19-5
	RIGHT
IN-LANE


17
	RIGHT
OUTLANE

27
	TROUGH

BALL

6

37
	LEFT
RAMP

DOWN


47
	MIDDLE
SKILL
SHOT

57
	BEHIND
LEFT
GOFER

67
	ADVANCE
TRAP
VALUE

 77
	NOT
USED

87
	Black-Gray

J208-10

Upper Left
Flipper E.O.S.

 F7

	Normal          

Function Volume Up
	Test
Function
Up
	
	
	
	
	
	
	
	
	
	

	D7
	
	
	
	
	
	
	
	
	
	

	Orange-Grey
J205-9           U16-5
	8

White​-
Grey
J208-9

U19-7
	BALL
SHOOTER

18
	KICK
BACK

28
	JET
POPPER

38
	RIGHT
RAMP
DOWN


48
	LOWER
SKILL
SHOT

58
	HOLE-IN
ONE
MADE

68
	SAND
TRAP

EJECT

78
	NOT
USED

88
	Black-Blue
J212-9
Upper Left
Flipper Opto

F8

	Normal          

Function  Begin Test
	Test
Function
Enter
	
	
	
	
	
	
	
	
	
	

	D8
	
	
	
	
	
	
	
	
	
	


        J2XX = CPU Board
= OPTO, TYPICALLY CLOSED















































































