WHITEWATER  (50018)
FUSE LIST

	POWER DRIVER BOARD
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	F101
	+50V DC General (Left Flipper)
	3A, 250V, SB Not Used
	

	F102
	+50V DC General (Right Flipper)
	3A, 250V, SB Not Used
	

	F103
	Solenoids #25 to #28
	3A, 250V, SB
	

	F104
	Solenoids #9 to #16
	3A, 250V, SB
	

	F105
	Solenoids #1 to #8
	3A, 250V, SB
	

	F106
	G.I. #5 White-Violet
	5A, 250V, SB
	

	F107
	G.I. #4 White-Green
	5A, 250V, SB
	

	F108
	G.I. #3 White-Yellow
	5A, 250V, SB
	

	F109
	G.I. #2 White-Orange
	5A, 250V, SB
	

	F110
	G.I. #1 White-Brown
	5A, 250V, SB
	

	F111
	Flasher Secondary
	5A, 250V, SB
	

	F112
	Solenoid Secondary 
	7A, 250V, SB
	

	F113
	+5V Logic
	5A, 250V, SB
	

	F114
	+18V Lamp Matrix
	8A, 32V, N.B.
	

	F115
	+12V Switch Matrix
	3/4A, 250V, FB
	

	F116
	+12V Secondary
	3A, 250V, SB
	

	Audio Board
	

	F501
	-25V Circuit
	3A, 250V, SB
	

	F502
	+25V Circuit
	3A, 250V, SB
	

	Dot Matrix Controller Board
	

	F601
	+62V Circuit
	3/8A, 250V, FB
	Fliptronic II Controller Board

	F602
	-113V & -125V Circuits
	3/8A, 250V, FB
	F901
	Upper Right Flipper
	3A, 250V, SB

	LINE FILTER
	F902
	Upper Left Flipper
	3A, 250V, SB

	Foreign
	
	5A, 250V, SB
	F903
	Lower Right Flipper
	3A, 250V, SB

	Domestic
	
	8A, 250V, SB
	F904
	Lower Left Flipper
	3A, 250V, SB


SOLENOID/FLASHER TABLE

	Sol
No.
	Function
	Solenoid
Type
	Voltage Connections
	Drive
Xistor
	Drive Connections
	Drive
Wire
Color
	Solenoid Part Number
Flashlamp Type

	
	
	
	Playfield
	Backbox
	Cabinet
	
	Playfield
	Insert
	Cabinet
	
	Playfield
	Insert

	01
	OUTHOLE
	High Power
	J107-3
	
	
	Q82
	J130-1
	
	
	VIO-BRN
	AE-27-1200
	

	02
	BALL SERVE
	High Power
	J107-3
	
	
	Q80
	J130-2
	
	
	VIO-RED
	AE-26-1200
	

	03
	WHIRLPOOL POPPER
	High Power
	J107-3
	
	
	Q78
	J130-4
	
	
	VIO-ORG
	AE-23-800
	

	04
	LOCKUP POPPER
	High Power
	J107-3
	
	
	Q76
	J130-5
	
	
	VIO-YEL
	AE-23-800
	

	05
	KICKBACK
	High Power
	J107-3
	
	
	Q64
	J130-6
	
	
	VIO-GRN
	AE-23-800
	

	06
	RAMP DIVERTER
	High Power
	J107-3
	
	
	Q66
	J130-7
	
	
	VIO-BLU
	AE-26-1200
	

	07
	KNOCKER
	High Power
	J107-3
	
	
	Q68
	J130-8
	
	
	VIO-BLK
	AE-23-800
	

	08
	BACKGLASS (2)
	High Power
	
	J106-5
	
	Q70
	
	J131-5
	
	VIO-GRY
	
	#906 (2)

	09
	WET WILLIE HEAD
	Low Power
	
	J106-5
	
	Q58
	
	J129-1
	
	BRN-BLK
	
	#906

	10
	LEFT SLING
	Low Power
	J107-2
	
	
	Q56
	J127-3
	
	
	BRN-RED
	AE-27-1200
	

	11
	RIGHT SLING
	Low Power
	J107-2
	
	
	Q54
	J127-4
	
	
	BRN-ORG
	AE-27-1200
	

	12
	LEFT JET BUMPER
	Low Power
	J107-2
	
	
	Q52
	J127-5
	
	
	BRN-YEL
	AE-26-1200
	

	13
	RIGHT JET BUMPER
	Low Power
	J107-2
	
	
	Q50
	J127-6
	
	
	BRN-GRN
	AE-26-1200
	

	14
	CENTER JET BUMPER
	Low Power
	J107-2
	
	
	Q48
	J127-7
	
	
	BRN-BLU
	AE-26-1200
	

	15
	BACKGLASS RAFT
	Low Power
	
	J106-5
	
	Q46
	
	J128-3
	
	BRN-VIO
	
	#906 (2)

	16
	BACKGLASS RIDERS
	Low Power
	
	J106-5
	
	Q44
	
	J128-5
	
	BRN-GRY
	
	#906 (2)

	17
	BIGFOOT BODY
	Flasher
	J107-6
	J106-5
	
	Q42
	J126-1
	J125-1
	
	BLK-BRN
	#89
	#906

	18
	RIGHT MOUNTAINS
	Flasher
	J107-6
	J106-5
	
	Q40
	J126-2
	J125-2
	
	BLK-RED
	#89
	#906

	19
	LEFT MOUNTAINS
	Flasher
	J107-6
	
	
	Q38
	J126-3
	
	
	BLK-ORG
	#89
	 - 

	20
	UPPER LEFT PLAYFIELD
	Flasher
	J107-6
	J106-5
	
	Q36
	J126-4
	J125-5
	
	BLK-YEL
	#89
	#906

	21
	INSANITY FALLS
	Flasher
	J107-6
	
	
	Q28
	J126-5
	
	
	BLU-GRN
	#89
	-

	22
	WHIRLPOOL POPPER
	Flasher
	J107-6
	
	
	Q30
	J126-6
	
	
	BLU-BLK
	#89
	-

	23
	WHIRLPOOL ENTER
	Flasher
	J107-6
	
	
	Q34
	J126-7
	
	
	BLU-VIO
	#89
	-

	24
	BIGFOOT CAVE
	Flasher
	J107-6
	J106-5
	
	Q32
	J126-8
	J125-9
	
	BLU-GRY
	#89
	#906

	25
	BIGFOOT DRIVE
	Low Power
	J107-1
	
	
	Q26
	J122-1
	
	
	BLU-BRN
	A-15680
	

	26
	BIGFOOT ENABLE
	Low Power
	J118-2,3
	
	
	Q24
	J122-2
	
	
	BLU-RED
	A-15680
	

	27
	CHASE LAMP CLOCK
	Low Power
	
	J105-4,5; J118-2,3
	Q22
	
	J123-4
	
	BLU-ORG
	A-15761
	

	28
	CHASE LAMP DATA
	Low Power
	
	J105-4,5; J118-2,3
	Q20
	
	J123-5
	
	BLU-YEL
	A-15761
	

	  General Illumination
	
	Voltage Connections
	Drive Xistor
	Drive Connections
	Drive
Wire
	Bulb Type

	
	
	Playfield
	Backbox
	Cabinet
	
	Playfield
	Backbox
	Cabinet
	
	Playfield
	Backbox

	01
	PLAYFIELD UPPER
	G.I.
	J120-1
	
	
	Q18
	J121-7
	
	
	WHT-BRN
	#555
	#555

	02
	PLAYFIELD CENTER
	G.I.
	J120-2
	
	
	Q10
	J121-8
	
	
	WHT-ORG
	#555
	#555

	03
	PLAYFIELD LOWER
	G.I.
	J120-3
	J121-3
	
	Q14
	J121-9
	J120-9
	
	WHT-YEL
	#555
	#555

	04
	BACKGLASS BOAT
	G.I.
	
	J121-5
	
	Q16
	
	J120-10
	
	WHT-GRN
	
	#555

	05
	BACKGLASS SKY
	G.I.
	
	J121-6
	J119-3
	Q12
	
	J120-11
	J119-1
	WHT-VIO
	
	#555

	  Flipper Circuits
	
	Playfield Voltage Connection
	Drive Transistors
	Playfield  Drive
	Drive Wire Colors
	Coil
Part No.
	Coil
Colors

	
	
	
	Power
	Hold
	Connections
	 Power
Hold
	
	

	
	LOWER LEFT FLIPPER
	Flipper
	J907-6, 7 (GRY-YEL)
	Q3
	Q9
	J902-7, 9
	BLU-GRY
ORG-BLU
	FL-15629
	BLUE

	
	LOWER RIGHT FLIPPER
	Flipper
	J907-8, 9 (BLU-YEL)
	Q4
	Q11
	J902-11, 13
	BLU-VIO
ORG-GRN
	FL-15629
	BLUE

	
	UPPER RIGHT FLIPPER
	Flipper
	J907-4, 5 (BLU-YEL)
	Q2
	Q7
	J902-4, 6
	BLK-BLU   ORG-VOI
	FL-11630
	RED



LAMP MATRIX
Red 
Yellow (B+)
16-10213
	     Column

Row
	1

Yellow-
Brown
J137-1

Q98
	2

Yellow-
Red
J137-2

Q97
	3

Yellow-
Orange
J137-3

Q96
	4

Yellow-
Black
J137-4

Q95
	5

Yellow-
Green
J137-5

Q94
	6

Yellow-
Blue
J137-6

Q93
	7

Yellow-
Violet
J137-7

Q92
	8

Yellow-
Gray
J137-8

Q91

	1

Red-
Brown
J133-1 Q90
	SHOOT

AGAIN

   11
	RIVER

1ST  “R”

21
	RAFT

7

  31
	3-BANK
CENTER

41
	HAZARD

1

51
	RAFT

1

61
	WHIRLPOOL

1

71
	LIGHT 

EXTRA

BALL

81

	2

Red-
Black
J133-2 Q89


	KICKBACK


12
	RIVER

“I”

22
	RAFT

8

32
	3-BANK

LOWER

42
	HAZARD

5

52
	RAFT

2

62
	WHIRLPOOL

2

72
	ADVANCE

RAFT

82

	3

Red-
Orange
J133-4 Q88


	LEFT

OUTLANE

13
	RIVER

“V”

23
	WET

WILLIE

33
	LOCK

RELEASE

43
	HAZARD

6

53
	RAFT

3

63
	WHIRLPOOL

3

73
	MYSTERY

83

	4

Red-
Yellow
J133-5 Q87


	LEFT
FLIPPER

LANE

14
	RIVER

“E”

24
	RAMP

MILLIONS

34
	3-BANK

TOP

44
	HAZARD

7

54
	RAFT

4

64
	WHIRLPOOL

4

74
	BOLDER 5 X

AWARD

84

	5

Red-
Green
J133-6 Q86


	RIGHT
FLIPPER

LANE

15
	RIVER

2ND “R”

25
	HAZARD

5

35
	HAZARD

4

45
	WHIRLPOOL

LIT

55
	RAFT

5

65
	WHIRLPOOL

5

75
	NOT

USED

85

	6

Red-
​Blue
J133-7 Q85


	RIGHT
OUTLANE

16
	HAZARD

3

26
	LEFT LIGHT

LOCK

36
	RIGHT LIGHT

LOCK

46
	EXTRA

BALL

56
	RAFT

6

66
	WHIRLPOOL

6

76
	NOT

USED

86

	7

Red​-
Violet
J133-8 Q84


	LIGHTS

WHIRLPOOL

17
	LOCK

1

27
	2 X

MULTIPLIER

37
	4 X

MULTIPLIER

47
	WHIRL

CHALLENGE

57
	2-BANK

UPPER

67
	MULTI

JACKPOT

77
	NOT

USED

87

	8

Red​-
Grey
J133-9 Q83


	6 X

MULTIPLIER

18
	LOCK

2

28
	3 X

MULTIPLIER

38
	5 X

MULTIPLIER

48
	BOLDER 

MAN

OVER

58
	2-BANK

LOWER

68
	BIGFOOT

JACKPOT

78
	START

BUTTON

88


        J1XX = Power Driver Board


SWITCH MATRIX
White
Green
	DEDICATED
GROUNDED
SWITCHES
	     Column

Row
	1

Green-
Brown
J207-1

U20-18
	2

Green-
Red
J207-2

U20-17
	3

Green-
Orange
J207-3

U20-16
	4

Green-
Yellow
J207-4

U20-15
	5

Green-
Black
J207-5

U20-14
	6

Green-
Blue
J207-6

U20-13
	7

Green-
Violet
J207-7

U20-12
	8

Green-
Grey
J207-9

U20-11
	FLIPPER
GROUNDED

SWITCHES

	Orange-Brown
J205-1
LEFT COIN
CHUTE
U17-5

D1
	1

White-
Brown
J209-1

U18-11
	NOT
USED

11
	SLAM
TILT

21
	RIVER

2ND “R”

31
	LIGHT LOCK

LEFT

41
	LEFT 

SLING

51
	WHIRL

POOL

POPPER

61
	RAPIDS

RAMP

MAIN

71
	NOT

USED

81
	BLACK-GREEN
J906-1


LOWER RIGHT
E.O.S. SWITCH

F1

	Orange-Red
J205-2
CENTER COIN
CHUTE
U17-7

D2
	2

White-
Red
J209-2

U18-9
	NOT
USED


12
	COIN
DOOR
CLOSED

22
	RIVER

“E”

32
	LIGHT LOCK

RIGHT

42
	RIGHT

SLING

52
	WHIRL

POOL

EXIT

62
	NOT

USED

72
	NOT

USED

82
	BLUE-VIOLET
J905-1


LOWER RIGHT
FLIPPER OPTO

F2

	Orange-Black
J205-3
RIGHT COIN
CHUTE
U17-11
D3
	3

White-
Orange
J209-3

U18-5
	START
BUTTON

13
	TICKET
OPTO.

23
	RIVER

“V”

33
	LEFT

LOOP

43
	BALL

SHOOTER


53
	LOCKUP

RIGHT

63
	HOT

FOOT

UPPER

73
	NOT

USED


83
	BLACK-BLUE

J906-3

LOWER LEFT
E.O.S. SWITCH

F3

	Orange-Yellow
J205-4
4TH COIN
CHUTE
U17-9

D4
	4

White-
Yellow
J209-4

U18-7
	PLUMB
BOB
TILT

14
	ALWAYS
CLOSED

24
	RIVER

“I”

34
	RIGHT

LOOP

44
	LOWER

JET

ARENA

54
	LOCKUP

CENTER

64
	HOT

FOOT

LOWER

74
	NOT

USED

84
	BLUE-GRAY

J905-2

LOWER LEFT
FLIPPER OPTO

F4

	Orange-Green
J205-6
	5

White-
Green
J209-5

U19-11
	OUTHOLE

15
	LEFT

OUTLANE

25
	RIVER

1ST “R”


35
	SECRET

PASSAGE


45
	RIGHT

JET

ARENA

55
	LOCKUP

LEFT

65
	DISASTER

DROP

MAIN

75
	NOT

USED


85
	BLACK-VIOLET

J906-4

UPPER RIGHT

E.O.S. SWITCH

F5

	Normal

Function

Srv Crdts
	Test

Function

Escape
	
	
	
	
	
	
	
	
	
	

	D5
	
	
	
	
	
	
	
	
	
	

	Orange-Blue
J205-7
	6

White-
​Blue
J209-7

U19-9
	LEFT 

JET

BUMPER

16
	LEFT FLIPPER

LANE

26
	3-BANK

TOP

36
	LEFT

RAMP

ENTER

46
	EXTRA

BALL

56
	LEFT

RAMP

MAIN

66
	RIGHT
TROUGH

76
	BIGFOOT

OPTO

1

86
	BLACK-YELLOW
J905-3

UPPER RIGHT
FLIPPER OPTO

F6

	Normal

Function

Volume Dn
	Test
Function

Down
	
	
	
	
	
	
	
	
	
	

	D6
	
	
	
	
	
	
	
	
	
	

	Orange-Violet
J205-8
	7

White​-
Violet
J209-8

U19-5
	RIGHT 

JET

BUMPER

17
	RIGHT

FLIPPER

LANE

27
	3-BANK

CENTER

37
	RAPIDS

ENTER

47
	CANYON

MAIN


57
	NOT

USED

67
	CENTER

TROUGH

 77
	BIGFOOT

OPTO

2

87
	BLACK-GRAY

J906-5

UPPER LEFT
E.O.S. SWITCH

F7

	Normal

Function

Volume Up
	Test
Function
Up
	
	
	
	
	
	
	
	
	
	

	D7
	
	
	
	
	
	
	
	
	
	

	Orange-Grey
J205-9
	8

White​-
Grey
J209-9

U19-7
	CENTER

JET

BUMPER

18
	RIGHT

OUTLANE

28
	3-BANK

LOWER

38
	CANYON

ENTRANCE

48
	BIGFOOT

CAVE


58
	DISASTER

DROP

ENTER

68
	LEFT

TROUGH

78
	NOT

USED

88
	BLACK-BLUE
J905-5

UPPER LEFT
FLIPPER OPTO

F8

	Normal

Function

Begin Test
	Test
Function
Enter
	
	
	
	
	
	
	
	
	
	

	D8
	
	
	
	
	
	
	
	
	
	


        J2XX = CPU Board
= OPTO, TYPICALLY CLOSED



























































































































































































